version: 8
hash: "zYkLN9+x1l99IXxN5uVR4Q=="
description: "DMP"
time_zone: "America/Chicago"
computer_name: "VFC-01-ABRQ"
network_device {
  number: 0
  name: "usb0"
  deprecated_version_1_dhcp_enable: false
  deprecated_version_1_ip_address: "192.168.240.2"
  deprecated_version_1_gateway: "192.168.240.1"
  deprecated_version_1_subnet_mask: "255.255.255.0"
  dns {
    deprecated_version_2_auto_obtain: false
    address {
      number: 0
      address: "192.168.240.1"
    }
  }
  mac: "4e:cb:59:41:eb:aa"
  static_ip {
    ip_address: "192.168.240.2"
    gateway: "192.168.240.1"
    subnet_mask: "255.255.255.0"
  }
}
network_device {
  number: 1
  name: "eth0"
  deprecated_version_1_dhcp_enable: true
  deprecated_version_1_ip_address: "0.0.0.0"
  deprecated_version_1_gateway: "0.0.0.0"
  deprecated_version_1_subnet_mask: "255.255.255.0"
}
network_device {
  number: 2
  name: "eth1"
  deprecated_version_1_dhcp_enable: false
  deprecated_version_1_ip_address: "172.16.192.25"
  deprecated_version_1_gateway: "0.0.0.0"
  deprecated_version_1_subnet_mask: "255.255.0.0"
  mac: "0a:ee:b3:dd:aa:e4"
  static_ip {
    ip_address: "172.16.192.25"
    subnet_mask: "255.255.0.0"
  }
}
sensor {
  type: Temperature
  number: 1
  temp_sensor {
    type: Ambient
    address: 4
    offset: 0
  }
}
client {
  type: Fusion
  number: 0
  enabled: false
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 443
        scheme: Https
        host: ""
        path: "/discovery-proxy/"
      }
    }
  }
}
client {
  type: Ntp
  number: 1
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Ntp
      ntp {
        host: "0.daktronics.pool.ntp.org"
      }
    }
  }
  transport {
    type: Ip
    number: 1
    ip {
      type: Ntp
      ntp {
        host: "1.daktronics.pool.ntp.org"
      }
    }
  }
  transport {
    type: Ip
    number: 2
    ip {
      type: Ntp
      ntp {
        host: "2.daktronics.pool.ntp.org"
      }
    }
  }
  transport {
    type: Ip
    number: 3
    ip {
      type: Ntp
      ntp {
        host: "3.daktronics.pool.ntp.org"
      }
    }
  }
}
client {
  type: SystemControl
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 85
        scheme: Http
        host: "192.168.240.1"
        path: ""
      }
    }
  }
}
service {
  type: Ntcip
  number: 0
  enabled: true
  ntcip {
    sign_count: 1
    lcd_menus_enabled: true
    display_menus_on_output: true
    generate_ttable: true
  }
}
service {
  type: Config
  number: 1
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 4500
        scheme: Http
        host: ""
        path: "/daktronics/config/1.0"
      }
    }
  }
}
service {
  type: Status
  number: 2
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 4501
        scheme: Http
        host: ""
        path: "/daktronics/status/1.0"
      }
    }
  }
}
service {
  type: PlayerControl
  number: 3
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 4502
        scheme: Http
        host: ""
        path: "/daktronics/playcontrol/1.0"
      }
    }
  }
}
service {
  type: Security
  number: 4
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 4503
        scheme: Http
        host: ""
        path: "/daktronics/security/1.0"
      }
    }
  }
}
service {
  type: Image
  number: 5
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 4505
        scheme: Http
        host: ""
        path: "/daktronics/imaging/1.0"
      }
    }
  }
}
service {
  type: Capabilities
  number: 6
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 4508
        scheme: Http
        host: ""
        path: "/daktronics/capabilities/1.0"
      }
    }
  }
}
service {
  type: PlayerData
  number: 7
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 4508
        scheme: Http
        host: ""
        path: "/daktronics/dataservice/1.0"
      }
    }
  }
}
service {
  type: FileTransfer
  number: 8
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 4508
        scheme: Http
        host: ""
        path: "/daktronics/fileservice/1.0"
      }
    }
  }
}
service {
  type: Updater
  number: 9
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 40005
        scheme: Http
        host: ""
        path: "/daktronics/updater/1.0"
      }
    }
  }
}
service {
  type: Management
  number: 10
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 80
        scheme: Http
        host: ""
        path: "/daktronics/management/1.0"
      }
    }
  }
}
service {
  type: ResourceUpdated
  number: 11
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 9999
        scheme: Http
        host: ""
        path: "/daktronics/resourceupdated/1.0"
      }
    }
  }
}
service {
  type: Layout
  number: 12
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 4508
        scheme: Http
        host: ""
        path: "/daktronics/layoutservice/1.0"
      }
    }
  }
}
service {
  type: Preview_v2
  number: 13
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 4508
        scheme: Http
        host: ""
        path: "/daktronics/preview/v2"
      }
    }
  }
}
service {
  type: Registration
  number: 14
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 4508
        scheme: Http
        host: ""
        path: "/daktronics/registration/1.0"
      }
    }
  }
}
service {
  type: CgControl
  number: 15
  enabled: true
  transport {
    type: Ip
    number: 0
    ip {
      type: Http
      http {
        port: 33309
        scheme: Http
        host: ""
        path: "/daktronics/cgcontrol"
      }
    }
  }
}
output {
  type: Display
  display {
    resolution {
      height: 720
      width: 1280
    }
    sign {
      number: 0
      video_loop: true
      preload_time: 0
      rect {
        top: 0
        left: 0
        height: 720
        width: 1280
      }
      name: "primary"
      audio_enabled: false
      default_content_enabled: false
      ui_meta {
        name: "ConfigEditMode"
        value: "SingleRect"
      }
      fit {
        mode: FitModeNotSpecified
        interpolation: Auto
      }
      background {
        color: "#00000000"
      }
    }
    audio {
      delay: "P0D"
      stream_offset: "P0D"
      clip_normalization {
        enabled: false
      }
      mono: false
      mute_fade_duration: "P0D"
    }
    device_id: "dev://sdl/0"
    refresh {
      numerator: 60
      denominator: 1
    }
    scan: Progressive
    keying: Off
    viewport {
      view {
        source {
          left: 0
          top: 0
          width: 1280
          height: 720
        }
        destination {
          left: 0
          top: 0
          width: 1280
          height: 720
        }
        sign_name: "primary"
        blend_mode: SourceOver
        rotation: 0
      }
    }
    fps {
      numerator: 3
      denominator: 1
    }
    pixel_format: "Unknown"
    color {
      color_transfer {
        type: sRGB
        sdr_mapping {
          mode: Auto
          nominal_peak_luminance: 1000
          white_level: "0.75"
        }
      }
    }
    streaming {
      streamSelect: multicast
      url: ""
      encryptedStreamKey: ""
      codec: "h264"
      bitrate: 3000
      profile: main
      level: "4.1"
      bFrames: 2
      rateControl: cbr
      referenceFrames: 1
      useHardwareEncoding: false
    }
  }
}
rtd {
  gip_source {
    dsrc: "AS5-Basketball"
    enabled: false
  }
}
watchdog {
  process {
    number: 0
    enabled: false
    path: "/usr/sbin/dak-player"
    weak: false
  }
  process {
    number: 1
    enabled: true
    path: "dak-vnet"
    weak: false
  }
}
ping_enabled: true
machine_id: "01ba4523-3c06-493a-a5e8-c49fe0592872"
reset_required: false
macro_group {
  name: "allsport"
  zone: "primary"
  macro {
    name: "1"
    content {
      number: 0
      filename: "basketball.vmpf"
    }
  }
  macro {
    name: "2"
    content {
      number: 0
      filename: "volleyball.vmpf"
    }
  }
  macro {
    name: "3"
    content {
      number: 0
      filename: "wrestling.vmpf"
    }
  }
  macro {
    name: "4"
    content {
      number: 0
      filename: "hockey.vmpf"
    }
  }
  macro {
    name: "5"
    content {
      number: 0
      filename: "baseball.vmpf"
    }
  }
  macro {
    name: "6"
    content {
      number: 0
      filename: "football.vmpf"
    }
  }
  macro {
    name: "7"
    content {
      number: 0
      filename: "soccer.vmpf"
    }
  }
  macro {
    name: "8"
    content {
      number: 0
      filename: "track.vmpf"
    }
  }
}
sshEnabled: true
