## DMP

## Computer Name: DAK-VFC-DEB12

Created On: Jan-27-2026, 10:44 AM

## 1. Network

No. | Name | DHCP Enable | IP Address | Gateway | Subnet mask | DNS Auto | DNS Domain
--- | --- | --- | --- | --- | --- | --- | ---
0 | usb0 | false | 192.168.240.2 | 192.168.240.1 | 255.255.255.0 | false |
1 | eth1 | false | 172.16.192.25 |  | 255.255.0.0 | true |

## 2. Display

No. | Frame Rate | Output Height | Output Width | Device Id | Keying | Scan | Output Count
--- | --- | --- | --- | --- | --- | --- | ---
0 | 60.00 | 720 | 1280 | dev://sdl/0 | off | progressive |

primary (sign 0)
Height | Width | Mode
--- | --- | ---
720 | 1280 | SingleRect

Output Location
X-Coordinate | Y-Coordinate | Rotation
--- | --- | ---
0 | 0 | 0

## 3. Clock

Time Zone
America/Chicago

## 4. RTD

Signs
No. | Sign ID
--- | ---

Data Source
No. | DSRC
--- | ---

## 5. Servers

Venus
Enabled | Host | Port
--- | --- | ---

## 6. Audio

Audio Enabled
false

## 7. Output Visual - Listed as WxH

### Output: 0

0 : primary (0,0 1280x720) => (0,0 1280x720)
0